1D Handfree

**Barcode Scanner**

**XL-6500A**

◎ Rugged and stylish design.

◎ Quick and ﬂuent reading performance.

◎ Laser scanner with auto scan and bracket.

◎ Bracket disassembled to saving shipping cost.

◎ With IP54 waterproof and dustproof protection.

|  |  |  |  |
| --- | --- | --- | --- |
| Model Number | XL-6500A | Size | L × W × H:175mm × 73mm × 102mm |
| Light Source | Visible Laser Diode 650nm | Weight | 246g |
| Scan Pattern | Single Scan | Material | ABS+PC |
| Decode Rate | 300 times/second | Voltage | 5VDC |
| Scan Precision | 3mil | Operating Current | 85mA |
| Scan Width | 30mm@scan window, 220mm@200mm | Static Current | 30mA |
| Scan Depth of ﬁeld | 0-330mm (0.33mm pcs0.9) | Laser Class | Meet the Grade I National Criteria for Laser Safety |
| Elevation Angle | 65 | EMC | CE& FCC DOC compliance |
| Deﬂection Angle | 55 | Operating Temperature | - 0°C to 50°C |
| Support Interface | PS-2(KB); RS-232; USB-HID; USB-Virtual COM | Storage Temperature | - 40°C to 70°C |
| Print Contrast | 10% UPC/EAN 100% | Humidity | 5% to 85% relative humidity,non-condensing |
| Mention Pattern | Buzzer, Indicator | Light Levels | Daylight,3000-8000LUX |
| Scan Mode | Automatic & Manual & Continuous | Shock | Designed to withstand 1.5M drops |
| Decoding Capability | EAN-8/EAN-13/UPC-A/UPC-E/Code 39/Code 93/Code 128/EAN128/Codaber/Industoal 2 of 5/Interleave 2 of 5/ Matrix 2 of 5/MSI。 | | |